For 1990-2009 cars

## Scan Tool Output Controls Except Holden

Scan Tool Output Control | Additional Menu Selections | Description
--- | --- | ---
ABS Lamp | Lamp Test | Commands the lamp ON and OFF
Automated Bleed | -- | Used in order to bleed the ABS hydraulics
Brake Warning Lamp | Lamp Test | Commands the lamp ON and OFF
Left Front Solenoid Valve Test | Solenoid Test | Commands the solenoid ON and OFF
Left Rear Solenoid Valve Test | Solenoid Test | Commands the solenoid ON and OFF
Pump Motor Test | -- | Commands the pump motor ON and OFF
Right Front Solenoid Valve Test | Solenoid Test | Commands the solenoid ON and OFF
Right Rear Solenoid Valve Test | Solenoid Test | Commands the solenoid ON and OFF

## Scan Tool Output Controls Holden

Scan Tool Output Control | Additional Menu Selections | Description
--- | --- | ---
Return Pump Relay Test | Chassis / Actuator Test | This function controls the Return Pump Relay. ON / OFF.
Front Left Solenoid Valve Test | Chassis / Actuator Test | This function controls the Front Left Solenoid Valve. ACTIVE / INACTIVE.
Front Right Solenoid Valve Test | Chassis / Actuator Test | This function controls the Front Righ Solenoid Valve. ACTIVE / INACTIVE.
Rear Left Solenoid Valve Test | Chassis / Actuator Test | This function controls the Rear Solenoid Valve. ACTIVE / INACTIVE.
Rear Right Solenoid Valve Test | Chassis / Actuator Test | This function controls the Rear Right Solenoid Valve. ACTIVE / INACTIVE.
Front Left TC Valve Test | Chassis / Actuator Test | This function controls the Front Left TC Valve . ACTIVE / INACTIVE.
Front Right TC Valve Test | Chassis / Actuator Test | This function controls the Front Right TC Valve. ACTIVE / INACTIVE.