For 1990-2009 cars

### Removal Procedure

1. Raise and support the liftgate in the open position.
2. Unscrew and remove the liftgate support from the liftgate and the body.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the liftgate support to the liftgate door and the body.

Tighten
Tighten the liftgate support studs to 8 N·m (71 lb in).

2. Close the liftgate.