For 1990-2009 cars

Warning: Refer to Safety Glasses Warning in the Preface section.

1. Clean the oil pump and the engine block gasket mating surface areas.
2. Remove the safety relief valve bolt.
3. Remove the safety relief valve and the spring.
4. Remove the oil pump-to-crankshaft seal.
5. Remove the oil pump rear cover bolts.
6. Remove the rear cover.
7. Clean the oil pump housing and all the oil pump parts.
8. Inspect all the oil pump parts for signs of wear. Refer to Engine Mechanical Specifications. Replace the worn oil pump parts.

Caution: Fill oil pump cavities with petroleum jelly prior to installation. This will ensure that there is oil pressure immediately on start-up and will prevent engine damage.

9. Coat all the oil pump parts with clean engine oil Install the oil pump parts.

Caution: Refer to Fastener Caution in the Preface section.

10. Apply Loctite® 242 to the oil pump rear cover bolts. Install the cover with the bolts and tighten to 6 N·m (53 lb in).
11. Install the safety relief valve, spring, washer and bolt. Tighten the valve bolt to 30 N·m (22 lb ft).