For 1990-2009 cars

#### Tools Required

• | 500-20 Hex Nut

• | J 2619-01 Slide Hammer

• | J 34866 Wheel Hub Remover

• | J 36661-2 Forcing Screw

• | J 37105-1 Support Bridge

• | J 37105-2 Bearing Adapter

• | J 37105-3 Hub Adapter

### Removal Procedure

1. Remove the steering knuckle and the hub as an assembly. Refer to Steering Knuckle Replacement .
2. Use a vise in order to hold the knuckle.
3. Place the J 34866 over 2 wheel studs.
4. Use 2 wheel nuts in order to secure the J 34866 to the wheel studs.
5. Install the J 2619-01 to the J 34866 .
6. Use the J 2619-01 in order to remove the hub from the knuckle.
7. Remove the brake shield. Refer to Front Brake Shield Replacement .
8. Remove the outer snap ring.
9. Remove the wheel bearing with the following tools:

• | J 37105-1 (1)

• | J 37105-2 (2)

• | 500-20 (4)

• | J 36661-2 (3)

10. Clean the bore of the knuckle.

### Installation Procedure

1. Install the outer snap ring and press the wheel bearing into place with the following tools:

• | J 37105-1 (4)

• | J 37105-2 (1)

• | 500-20 (2)

• | J 36661-2 (3)

2. Install the brake shield. Refer to Front Brake Shield Replacement .
3. Press the wheel hub into place with the following tools:

• | J 37105-3 (4)

• | J 37105-2 (1)

• | 500-20 (2)

• | J 36661-2 (3)

4. Install the drive axle into the front wheel hub. Refer to Steering Knuckle Replacement .