For 1990-2009 cars

### Circuit Description

When the ignition switch is turned to ON, the sensing and diagnostic module (SDM) will perform turn-on test to diagnose critical malfunctions within SDM itself.

Upon passing these test ignition and deployment loop voltages are measured to ensure that they are within their normal voltage ranges. The SDM monitors the voltages at the driver low and the passenger low to detect shorts to ground or voltage in the deploy loops.

The SDM checks the wiring connection to the passenger side airbag module by letting the infinitesimal current flow through the internal circuit and verify the resistance.

### DTC Descriptor

This diagnostic procedure supports the following DTC:

DTC B1384 RF Side Deployment Loop Short to Ground

### Conditions for Running the DTC

Ignition voltage is within the normal operating voltage range.

### Conditions for Setting the DTC

• | The side air bag wiring of the passenger high is shorted to ground.

• | The side air bag wiring of the passenger low is shorted to ground.

### Action Taken When the DTC Sets

The SDM commands the AIR BAG indicator ON.

### Conditions for Clearing the DTC

The condition responsible for setting the DTC no longer exists and the scan tool Clear DTCs function is used.

Step | Action | Values | Yes | No
--- | --- | --- | --- | ---
Caution: Refer to Sensing and Diagnostic Module Handling Caution in the Preface section. Caution: Refer to Sensing and Diagnostic Module Voltage after Ignition is Turned Off Caution in the Preface section. Schematic Reference: SIR Schematics Connector End View Reference: SIR Connector End Views
1 | Did you perform the Diagnostic System Check - Vehicle? | -- | Go to Step 2 | Go to Diagnostic System Check - Vehicle
2 |

1. Confirm the ignition switch is OFF.
2. Wait for 1 minute for the sensing and diagnostic module (SDM) charger to be discharged.

Has the SDM discharged?

∞

Go to Step 3

--

3 | Visually inspect any damage for the air bag wiring. Is the air bag wiring damaged? | -- | Go to Step 5 | Go to Step 4
4 | Measure the resistance between the high, low terminal of the passenger side impact module harness connector and ground. Is the resistance equal to the specified value? | 10 Kohms | Go to Step 6 | Go to Step 5
5 | Replace the air bag wiring. Is the replacement complete? | -- | Go to Step 8 | --
6 |

1. Replace the SDM. Refer to Inflatable Restraint Sensing and Diagnostic Module Replacement .
2. Confirm the ignition switch is ON.
3. Use the scan tool to clear the DTCs.
4. Perform the Diagnostic System Check - Vehicle .

Is the DTC removed?

--

Go to Step 8

Go to Step 7

7 | Replace the passenger side impact module. Is the replacement complete? | -- | Go to Step 8 | --
8 |

1. Reconnect all SIR system components.
2. Verify that all components, connectors, and connector position assurances (CPAs) are properly mounted.
3. Use the scan tool to clear the DTCs.
4. Operate the vehicle within the Conditions for Running the DTC as specified in the text.

Does the DTC reset?

--

Go to Step 2

System OK