For 1990-2009 cars

1. Install the oil pump drive gear and driven gear.
2. Align the stator shaft with each bolt hole.

Notice: Refer to Fastener Notice in the Preface section.

3. Install the 8 bolts.

Tighten
Tighten the bolts to 9.8 N·m (87 lb in).

Notice: Use extreme care when working around oil seals. Damage to the lip of a seal will cause oil leaks.

4. Turn the drive gear with 2 screwdrivers and make sure it rotates smoothly.