For 1990-2009 cars

### Removal Procedure

Note: The left-hand drive model is shown. The right-hand drive model is similar.

1. Remove the instrument panel (I/P). Refer to Instrument Panel Assembly Replacement.
2. Remove the nuts from the brace.
3. Remove the brake pedal.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the brace with the nuts and tighten to 22 N·m (16 lb ft).
2. Install the brake pedal.
3. Install the I/P. Refer to Instrument Panel Assembly Replacement.