For 1990-2009 cars

## Tail Lamp Replacement Five Door

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the tail lamp assembly screws.
3. Slide the tail lamp assembly toward the hatch opening and remove the tail lamp assembly.
4. Remove the bulbs.

### Installation Procedure

1. Install the bulbs.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the lamp assembly with the screws and tighten to 3 N·m (27 lb in).
3. Connect the negative battery cable.

## Tail Lamp Replacement Four Door

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the nuts and the lamp assembly.
3. Remove the bulbs.

### Installation Procedure

1. Install the bulbs.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the lamp assembly with the nuts and tighten to 4 N·m (35 lb in).
3. Connect the negative battery cable.

## Tail Lamp Replacement Wagon

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the tail lamp assembly screws.
3. Remove the tail lamp assembly.
4. Remove the bulbs.

### Installation Procedure

1. Install the bulbs.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the lamp assembly with the screws and tighten to 3 N·m (27 lb in).
3. Connect the negative battery cable.