For 1990-2009 cars

### Removal Procedure

Warning: Refer to Title not found in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the rear seat cushion. Refer to Rear Seat Cushion Replacement.
3. Remove the left and the right rear rocker trim panels. Refer to Rear Side Door Sill Plate Replacement.
4. Remove the bolts and the left and the right lower front seat belt anchors from the center pillar.
5. Remove the left and the right front rocker trim panels.
6. Remove the left and the right lower center pillar trim panels. Refer to Center Pillar Lower Trim Panel Replacement.
7. Remove the front seats. Refer to Front Seat Replacement - Bucket.
8. Remove the left and the right kick panels. Refer to Body Hinge Pillar Trim Panel Replacement.
9. Remove the floor console. Refer to Front Floor Console Replacement.
10. Remove the gearshift housing bolts and nuts and reposition the gearshift housing.
11. Remove the floor carpet.

### Installation Procedure

1. Install the floor carpet.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the gearshift housing with the bolts and tighten to 8 N·m (70 lb in).
3. Install the floor console. Refer to Front Floor Console Replacement.
4. Install the left and the right kick panels. Refer to Body Hinge Pillar Trim Panel Replacement.
5. Install the front seats. Refer to Front Seat Replacement - Bucket.
6. Install the left and the right lower center pillar trim panels. Refer to Center Pillar Lower Trim Panel Replacement.
7. Install the left and the right front rocker trim panels.
8. Install the left and the right lower front seat belt anchors to the center pillar with the bolts and tighten to 38 N·m (28 lb ft).
9. Install the left and the right rear rocker trim panels. Refer to Rear Side Door Sill Plate Replacement.
10. Install the rear seat cushion. Refer to Rear Seat Cushion Replacement.
11. Connect the negative battery cable.