For 1990-2009 cars

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the door trim panel. Refer to Front Side Door Trim Panel Replacement or Rear Door Trim Panel Replacement.
3. Disconnect the electrical connector.
4. Remove the screws and the door speaker.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the door speaker with the screws and tighten to 2 N·m (18 lb in).
2. Connect the electrical connector.
3. Install the door trim panel. Refer to Front Side Door Trim Panel Replacement or Rear Door Trim Panel Replacement.
4. Connect the negative battery cable.