For 1990-2009 cars

#### Tools Required

DT 46468 (DW260-020) Auto Transaxle Holding Fixture

Caution: Refer to Safety Glasses Caution in the Preface section.

Notice: Refer to Fastener Notice in the Preface section.

Caution: To reduce the possibility of personal injury or transmission damage install and tighten the support fixture bolts.

1. Install DT 46468 (1) onto the transaxle.

Tighten
Tighten the bolts to 11 N·m (98 lb in).

2. Position the transaxle with the rear cover facing up.