For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Diagnostic System Check - Vehicle? | -- | Go to Step 2 | Go to Diagnostic System Check - Vehicle
2 | With a fused jumper wire, connect terminals 4 and 5 of the fuel pump connector together. Did the Low Fuel Indicator turn ON? | -- | Go to Step 7 | Go to Step 3
3 | Using a multimeter, test terminal 4 of the fuel pump connector for continuity to ground. Refer to Testing for Continuity . Is ground present? | -- | Go to Step 4 | Go to Step 5
4 | Using a multimeter, test for continuity between terminal 5 of the fuel pump connector and terminal B14 of the instrument cluster. Refer to Testing for Continuity . Is continuity present? | -- | Go to Step 8 | Go to Step 6
5 | Repair the open in ground circuit between terminal 4 of the fuel pump and ground 302. Refer to Wiring Repairs . Did you find and complete the repair? | -- | Go to Step 9 | --
6 | Repair the open in signal circuit between terminal 5 of the fuel pump connector and terminal B14 of the instrument cluster. Refer to Wiring Repairs . Did you find and complete the repair? | -- | Go to Step 9 | --
7 | Replace the fuel pump assembly. Refer to one of the following:

• | Fuel Pump Replacement for the 1.4L engine.

• | Fuel Pump Replacement for the 1.6L engine.

• | Fuel Pump Replacement for the 1.8L (L79) engine.

• | Fuel Pump Replacement for the 1.8L (LDA) engine.

• | Fuel Pump Replacement for the 2.0L engine.

Did you complete the repair?

--

Go to Step 9

--

8 | Replace the instrument cluster assembly. Refer to Instrument Cluster Replacement Did you complete the repair? | -- | Go to Step 9 | --
9 | Operate the system in order to verify the repair. Did you find and complete the repair? | -- | System OK | Go to Step 2