For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Pry off the dome lamp lens by inserting a screwdriver into the recess along the edge of the lens.
3. Remove the screws and the dome lamp housing from the headliner.
4. Disconnect the electrical connector.
5. Remove the bulb.

### Installation Procedure

1. Install a new bulb.
2. Connect the electrical connector.

Notice: Refer to Fastener Notice in the Preface section.

3. Install the dome lamp housing to the headliner with the screws.
4. Press the dome lamp lens onto the housing.
5. Connect the negative battery cable.