For 1990-2009 cars

Position | Solenoid | Clutch | Brake | 1-Way Clutch
--- | --- | --- | --- | ---
Shift 1 | Shift 2 | Timing | C1 | C2 | C3 | B1 | B2 | B3 | F1 | F2
R | V is less than 9 km/h (5 mph) | ON | ON | ON | OFF | OFF | ON | OFF | OFF | ON | OFF | OFF
| V is greater than or equal to 9 km/h (5 mph) | ON | ON | ON | OFF | OFF | OFF | OFF | OFF | OFF | OFF | OFF

A. Front Planetary Gear

B. Rear Planetary Gear

#### Reverse Gear

1. The input shaft rotates clockwise.

The reverse clutch (C3) operates. Connect the input shaft to the rear planetary sun gear.

2. The planetary long pinion rotates itself counterclockwise.
3. The 1st and reverse brake (3) operates. Lock rotates the planetary carrier.
4. The ring gear rotates counterclockwise.
5. The counter drive gear rotates counterclockwise for the ring gear and one.
6. The counter driven gear rotates clockwise.
7. The differential gear drive pinion rotates clockwise for the counter driven gear and one.
8. The differential gear rotates counterclockwise.

#### Engine Brake

The driving force is connected to the input shaft directory without the 1-way clutch. Therefore the engine brake operates.