For 1990-2009 cars

## DTC P0106 w/o Throttle Actuator Control

### Diagnostic Instructions

• | Perform the Diagnostic System Check - Vehicle prior to using this diagnostic procedure.

• | Review Strategy Based Diagnosis for an overview of the diagnostic approach.

• | Diagnostic Procedure Instructions provides an overview of each diagnostic category.

### DTC Descriptor

DTC P0106: Manifold Absolute Pressure (MAP) Sensor Performance

### Diagnostic Fault Information

Circuit | Short to Ground | Open/High Resistance | Short to Voltage | Signal Performance
--- | --- | --- | --- | ---
5-Volt Reference | P0107 | P0107 | P0108 | P0106
MAP Sensor Signal | P0107 | P0107 | P0108 | P0106
Low Reference | -- | P0108, P2106, P2110 | -- | P0106

### Typical Scan Tool Data

#### MAP Sensor

Circuit | Short to Ground | Open | Short to Voltage
--- | --- | --- | ---
Operating Conditions: Engine operating in Closed Loop Parameter Normal Range: 32-48 kPa
5-Volt Reference | 10 kPa | 10 kPa | 50 kPa
MAP Sensor Signal | 10 kPa | 10 kPa | 104 kPa
Low Reference | -- | 98 kPa | 104 kPa¹
¹ Internal ECM damage may occur if the circuit is shorted to B+.

### Circuit/System Description

The manifold absolute pressure (MAP) sensor responds to pressure changes in the intake manifold. The pressure changes occur based on the engine load. The engine control module (ECM) supplies 5 volts to the MAP sensor on the 5-volt reference circuit. The ECM provides a ground on the low reference circuit. The MAP sensor provides a signal to the ECM on the MAP sensor signal circuit which is relative to the pressure changes in the manifold. The ECM detects a low signal voltage at a low MAP, such as during an idle or a deceleration. The ECM detects a high signal voltage at a high MAP, such as the ignition is ON, with the engine OFF, or at a wide open throttle (WOT). The MAP sensor is also used to determine the barometric pressure (BARO). This occurs when the ignition switch is turned ON, with the engine OFF. The BARO reading may also be updated whenever the throttle position (TP) sensor is greater than 28 percent.

### Condition for Running the DTC

• | DTCs P0107, P0108, P0115, P0117, P0118, P0122, P0123, P0125, P0201, P0202, P0203, P0204, P0300, P0351, P0352, P0401, P0402, P0404, P0405, P0406, P0443, P0488, P0496, P0506, P0507 are not set.

• | The engine is running.

• | Valid BARO update.

• | The traction control is not active.

• | The torque converter clutch (TCC) is steady (A/T).

• | The A/C compressor clutch is steady.

• | The coolant temperature (ECT) is greater than -10°C (14°F).

• | The engine speed is between 1,300-4,500 RPM.

• | The change in engine speed is less than 200 RPM.

• | The change in idle air is less than 5 percent.

• | The change in throttle position (TP) is less than 3 percent, or the change in MAP is less than 5 kPa.

• | The change in exhaust gas recirculation (EGR) position is less than 6 percent.

• | The above conditions are stabilized for 1.5 seconds.

• | The DTC runs continuously when the above conditions are met.

### Conditions for Setting the DTC

The ECM detects that the actual MAP signal is not within the predicted range for more than 15 seconds.

### Action Taken When the DTC Sets

DTC P0106 is a Type B DTC.

### Conditions for Clearing the MIL/DTC

DTC P0106 is a Type B DTC.

### Reference Information

#### Schematic Reference

Engine Controls Schematics

#### Connector End View Reference

• | Engine Control Module Connector End Views

• | Engine Controls Connector End Views

#### Electrical Information Reference

• | Circuit Testing

• | Connector Repairs

• | Testing for Intermittent Conditions and Poor Connections

• | Wiring Repairs

#### DTC Type Reference

Powertrain Diagnostic Trouble Code (DTC) Type Definitions

#### Scan Tool Reference

• | Scan Tool Data List

• | Scan Tool Data Definitions

• | Scan Tool Output Controls

### Circuit/System Verification

1. Ignition ON, observe the DTC information with a scan tool. DTCs P0107, P0108, P0122, or P0123 should not be set.

⇒ | If a DTC is set, refer to Diagnostic Trouble Code (DTC) List - Vehicle .

Important: In extreme cold weather conditions ice may form in the vacuum source to the MAP sensor and may set a DTC. Inspect the MAP sensor and the vacuum source for ice, moisture, or other restrictions.

2. Start the engine and observe the scan tool MAP sensor pressure parameter. The MAP sensor pressure parameter should change while starting the engine.
3. Engine idling, observe the scan tool MAP Sensor pressure parameter. The reading should be between 32-48 kPa.

Important: The vehicle used for the comparison is not limited to the same type of vehicle being serviced. A vehicle known to provide an accurate reading is acceptable.

4. Compare the MAP sensor pressure parameter to the pressure parameter of a known good vehicle. The reading should be within 3 kPa of the known good vehicle.

Important: The Altitude vs Barometric Pressure table indicates a pressure range for a given altitude under normal weather conditions. Weather conditions consisting of very low or very high pressure and/or very low or very high temperature may cause a reading to be slightly out of range.

5. Compare the MAP sensor pressure parameter to the reading in the Altitude Versus Barometric Pressure table . The MAP sensor pressure parameter should be within the specified range indicated on the table.
6. Snap the throttle while observing the MAP sensor pressure parameter on the scan tool. The MAP sensor pressure parameter should change rapidly when the throttle position changes.
7. If the vehicle passes the Circuit/System Verification test, then operate the vehicle within the conditions for running the DTC. You may also operate the vehicle within the conditions that are captured in the Freeze Frame/Failure Records List.

### Circuit/System Testing

1. Verify that none of the following conditions exist:

• | Vacuum leaks or restrictions at the MAP sensor.

• | Engine vacuum leaks.

• | Restricted exhaust--Refer to Restricted Exhaust .

• | Worn piston rings--Refer to Engine Compression Test .

• | Incorrect cam timing--Refer to Timing Belt Inspection for the correct timing.

2. Ignition OFF, disconnect the harness connector of the TP sensor.
3. Test for less than 5 ohms of resistance between the low reference circuit and ground.

⇒ | If greater than the specified value, test the low reference circuit for an open/high resistance. If the circuit/connections test normal, replace the ECM.

4. Ignition ON, verify that the scan tool TP sensor position sensor voltage parameter is less than 0.3 volt.

⇒ | If greater than the specified value, test the signal circuit for a short to voltage. If the circuit/connections tests normal, replace the ECM.

Important: The 5-volt reference circuits are internally and externally connected at the ECM. Other component DTCs may be set. If other DTCs are set, review the electrical schematic and diagnose the applicable circuits and components.

5. Load test for 4.8-5.2 volts between the 5-volt reference circuit and ground.

⇒ | If less than the specified range, test the 5-volt reference circuit for a short to ground or open/high resistance. If the circuit/connections test normal, replace the ECM.

⇒ | If greater than the specified range, test the 5-volt reference circuit for a short to voltage. If the circuit/connections test normal, replace the ECM.

6. Ignition OFF, connect the harness connector of the TP sensor.
7. Disconnect the harness connector of the MAP sensor.
8. Test for less than 5 ohms of resistance between the low reference circuit and ground.

⇒ | If greater than the specified value, test the low reference circuit for a short to voltage or an open/high resistance. If the circuit/connections test normal, replace the ECM.

9. Ignition ON, verify that the MAP sensor parameter is less than 12 kPa.

⇒ | If greater than the specified value, test the signal circuit for a short to voltage. If the circuit/connections test normal, replace the ECM.

Important: The 5-volt reference circuits are internally and externally connected at the ECM. Other component DTCs may be set. If other DTCs are set, review the electrical schematic and diagnose the applicable circuits and components.

10. Load test for 4.8-5.2 volts between the 5-volt reference circuit and ground.

⇒ | If less than the specified range, test the 5-volt reference circuit for a short to ground or open/high resistance. If the circuit/connections test normal, replace the ECM.

⇒ | If greater than the specified range, test the 5-volt reference circuit for a short to voltage. If the circuit/connections test normal, replace the ECM.

11. Install a 3-amp fused jumper wire between the signal circuit and the 5-volt reference circuit. Verify that the scan tool MAP sensor parameter is greater than 102 kPa.

⇒ | If less than the specified value, test the signal circuit for a short to ground or an open/high resistance. If the circuit/connections test normal, replace the ECM.

12. If all circuits/connections test normal, test or replace the MAP sensor.

### Component Testing

1. Ignition OFF, perform one of the following applicable procedures.

• | Disconnect the vacuum supply hose from the MAP sensor

• | Remove the MAP sensor from the intake manifold

2. Ignition ON, observe and record the scan tool MAP sensor pressure data parameter. This is the first MAP sensor reading.
3. With the J 23738-A apply 5 in Hg (17 kPa) of vacuum to the MAP sensor. Observe and record the scan tool MAP sensor pressure data parameter. This is the second MAP sensor reading.
4. Subtract the second MAP sensor reading from the first MAP sensor reading. Verify that the vacuum decrease is within 1 in Hg (4 kPa) of the applied vacuum.

⇒ | If the vacuum decrease is not within the specified range, replace the MAP sensor.

5. With the J 23738-A apply 10 in Hg (34 kPa) of vacuum to the MAP sensor. Observe and record the scan tool MAP sensor pressure data parameter. This is the third MAP sensor reading.
6. Subtract the third MAP sensor reading from the first MAP sensor reading. Verify that the vacuum decrease is within 1 in Hg (4 kPa) of the applied vacuum.

⇒ | If the vacuum is not with in the specified range, replace the MAP sensor.

### Repair Instructions

Perform the Diagnostic Repair Verification after completing the diagnostic procedure.

• | Manifold Absolute Pressure Sensor Replacement

• | Throttle Body Assembly Replacement

• | Control Module References for engine control module replacement, setup, and programming

## DTC P0106 w/ Throttle Actuator Control

### Diagnostic Instructions

• | Perform the Diagnostic System Check - Vehicle prior to using this diagnostic procedure.

• | Review Strategy Based Diagnosis for an overview of the diagnostic approach.

• | Diagnostic Procedure Instructions provides an overview of each diagnostic category.

### DTC Descriptor

DTC P0106: Manifold Absolute Pressure (MAP) Sensor Performance

### Diagnostic Fault Information

Circuit | Short to Ground | Open/High Resistance | Short to Voltage | Signal Performance
--- | --- | --- | --- | ---
5-Volt Reference | P0107, P0405, P0452, P0651, P2106, P2110 | P0107 | P0108, P0651, P2076 | P0106
MAP Sensor Signal | P0107 | P0107 | P0108 | P0106
Low Reference | -- | P0108, P2106, P2110 | -- | P0106

### Typical Scan Tool Data

#### MAP Sensor

Circuit | Short to Ground | Open | Short to Voltage
--- | --- | --- | ---
Operating Conditions: Engine operating in Closed Loop Parameter Normal Range: 32-48 kPa
5-Volt Reference | 10 kPa | 10 kPa | 50 kPa
MAP Sensor Signal | 10 kPa | 10 kPa | 104 kPa
Low Reference | -- | 98 kPa | 104 kPa¹
¹ Internal ECM damage may occur if the circuit is shorted to B+.

### Circuit/System Description

The manifold absolute pressure (MAP) sensor responds to pressure changes in the intake manifold. The pressure changes occur based on the engine load. The engine control module (ECM) supplies 5 volts to the MAP sensor on the 5-volt reference circuit. The ECM provides a ground on the low reference circuit. The MAP sensor provides a signal to the ECM on the MAP sensor signal circuit which is relative to the pressure changes in the manifold. The ECM detects a low signal voltage at a low MAP, such as during an idle or a deceleration. The ECM detects a high signal voltage at a high MAP, such as the ignition is ON, with the engine OFF, or at a wide open throttle (WOT). The MAP sensor is also used to determine the barometric pressure (BARO). This occurs when the ignition switch is turned ON, with the engine OFF. The BARO reading may also be updated whenever the TP sensor is greater than 28 percent.

### Condition for Running the DTC

• | DTCs P0107, P0108, P0110, P0111, P0112, P0113, P0116, P0117, P0118, P0125, P0217, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0300, P0335, P0336, P0351, P0352, P0444, P0445, P0502, P0562, P0563, or P2110 are not set.

• | The engine is running.

• | Valid BARO update.

• | The traction control is not active.

• | The torque converter clutch (TCC) is steady (A/T).

• | The A/C compressor clutch is steady.

• | The coolant temperature is more than -10°C (14°F).

• | The engine speed is between 1,300-4,500 RPM.

• | The change in engine speed is less than 200 RPM.

• | The change in idle air is less than 5 percent.

• | The change in throttle position (TP) is less than 3 percent, or the change in MAP is less than 5 percent.

• | The change in exhaust gas recirculation (EGR) position is less than 6 percent.

• | The above conditions are stabilized for 1.5 seconds.

• | The DTC runs continuously when the above conditions are met.

### Conditions for Setting the DTC

The ECM detects that the actual MAP signal is not within the predicted range for more than 15 seconds.

### Action Taken When the DTC Sets

DTC P0106 is a Type B DTC.

### Conditions for Clearing the DTC

DTC P0106 is a Type B DTC.

### Diagnostic Aids

• | If a shared 5-volt reference circuit is shorted to ground or shorted to a voltage, other 5-volt reference circuits may be affected.

• | The scan tool 5-volt reference parameter should display between 4.8-5.2 volts.

### Reference Information

#### Schematic Reference

Engine Controls Schematics

#### Connector End View Reference

• | Engine Control Module Connector End Views

• | Engine Controls Connector End Views

#### Electrical Information Reference

• | Circuit Testing

• | Connector Repairs

• | Testing for Intermittent Conditions and Poor Connections

• | Wiring Repairs

#### DTC Type Reference

Powertrain Diagnostic Trouble Code (DTC) Type Definitions

#### Scan Tool Reference

• | Scan Tool Data List

• | Scan Tool Data Definitions

• | Scan Tool Output Controls

### Circuit/System Verification

1. Ignition ON, observe the DTC information with a scan tool. Verify DTCs P0107, P0108 or P0651 are not set.

⇒ | If a DTC is set, refer to Diagnostic Trouble Code (DTC) List - Vehicle .

Important: In extreme cold weather conditions ice may form in the vacuum source to the MAP sensor and may set a DTC. Inspect the MAP sensor and the vacuum source for ice, moisture, or other restrictions.

2. Start the engine and observe the scan tool MAP sensor pressure parameter. The MAP sensor pressure parameter should change while starting the engine.
3. Engine idling, observe the scan tool MAP Sensor parameter. The reading should be between 32-48 kPa.

Important: The vehicle used for the comparison is not limited to the same type of vehicle being serviced. A vehicle known to provide an accurate reading is acceptable.

4. Compare the MAP sensor pressure parameter to the pressure parameter of a known good vehicle. The reading should be within 3 kPa of the known good vehicle.

Important: The Altitude vs Barometric Pressure table indicates a pressure range for a given altitude under normal weather conditions. Weather conditions consisting of very low or very high pressure and/or very low or very high temperature may cause a reading to be slightly out of range.

5. Compare the MAP sensor pressure parameter to the reading in the Altitude Versus Barometric Pressure table . The MAP sensor pressure parameter should be within the specified range indicated on the table.
6. Snap the throttle while observing the scan tool MAP sensor pressure parameter. The MAP sensor pressure parameter should change rapidly when the throttle position changes.
7. If the vehicle passes the Circuit/System Verification test, then operate the vehicle within the conditions for running the DTC. You may also operate the vehicle within the conditions that are captured in the Freeze Frame/Failure Records List.

### Circuit/System Testing

1. Verify that none of the following conditions exist:

| Important: In extreme cold weather conditions ice may form in the vacuum source to the MAP sensor and may set a DTC. Inspect the MAP sensor and the vacuum source for ice, moisture, or other restrictions.

• | Vacuum leaks or restrictions at the MAP sensor

• | Engine vacuum leaks

• | Leaking exhaust gas recirculation (EGR) valve

• | Restricted exhaust--Refer to Restricted Exhaust .

• | Worn piston rings--Refer to Engine Engine Compression Test .

• | Incorrect cam timing--Refer to Timing Belt Inspection for the correct timing.

2. Ignition OFF, disconnect the harness connector at the MAP sensor.
3. Ignition ON, test for less than 0.2 volt between the low reference circuit and ground.

⇒ | If greater than the specified value, test the low reference circuit for a short to voltage. If the circuit/connections test normal, replace the ECM.

4. Ignition OFF, test for less than 5 ohms of resistance between the low reference circuit and ground.

⇒ | If greater than the specified value, test the low reference circuit for an open/high resistance. If the circuit/connections test normal, replace the ECM.

5. Ignition ON, load test for 4.8-5.2 volts between the 5-volt reference circuit and ground.

⇒ | If less than 4.8 volts, test the 5-volt reference circuit for a short to ground or open/high resistance. If the circuit/connections test normal, replace the ECM.

⇒ | If greater than 5.2 volts, test the 5-volt reference circuit for a short to voltage. If the circuit/connections test normal, replace the ECM.

6. Verify that the MAP sensor parameter is less than 12 kPa.

⇒ | If greater than 12 kPa, test the signal circuit for a short to voltage. If the circuit/connections test normal, replace the ECM.

7. Install a 3-amp fused jumper wire between the signal circuit and the 5-volt reference circuit. Verify that the MAP sensor parameter is greater than 102 kPa.

⇒ | If less than 102 kPa, test the signal circuit for a short to ground or an open/high resistance. If the circuit/connections test normal, replace the ECM.

8. If all circuits/connections test normal, test or replace the MAP sensor.

### Component Testing

1. Ignition OFF, perform one of the following applicable procedures.

• | Disconnect the vacuum supply hose from the MAP sensor

• | Remove the MAP sensor from the intake manifold

2. Ignition ON, observe and record the scan tool MAP sensor pressure data parameter. This is the first MAP sensor reading.
3. With the J 23738-A apply 5 in Hg (17 kPa) of vacuum to the MAP sensor. Observe and record the scan tool MAP sensor pressure data parameter. This is the second MAP sensor reading.
4. Subtract the second MAP sensor reading from the first MAP sensor reading. Verify that the vacuum decrease is within 1 in Hg (4 kPa) of the applied vacuum.

⇒ | If the vacuum decrease is not within the specified range, replace the MAP sensor.

5. With the J 23738-A apply 10 in Hg (34 kPa) of vacuum to the MAP sensor. Observe and record the scan tool MAP sensor pressure data parameter. This is the third MAP sensor reading.
6. Subtract the third MAP sensor reading from the first MAP sensor reading. Verify that the vacuum decrease is within 1 in Hg (4 kPa) of the applied vacuum.

⇒ | If the vacuum is not with in the specified range, replace the MAP sensor.

### Repair Instructions

Perform the Diagnostic Repair Verification after completing the diagnostic procedure.

• | Manifold Absolute Pressure Sensor Replacement

• | Control Module References for ECM replacement, setup, and programming