For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Diagnostic System Check - Vehicle? | -- | Go to Step 2 | Go to Diagnostic System Check - Vehicle
2 | Disconnect the fuel pump connector . Did the Low Fuel Indicator turn OFF? | -- | Go to Step 5 | Go to Step 3
3 | Using a multimeter, test for a short to ground between terminal 5 of the fuel pump connector and terminal B14 of the instrument cluster. Refer to Testing for Short to Ground . Is ground present? | -- | Go to Step 4 | Go to Step 6
4 | Repair the short to ground in the signal circuit between terminal 5 of the fuel pump connector and terminal B14 of the instrument cluster. Did you find and complete the repair? | -- | Go to Step 7 | --
5 | Replace the fuel pump assembly. Refer to one of the following:

• | Fuel Pump Replacement

| for the 1.4L engine.

• | Fuel Pump Replacement

| for the 1.6L engine.

• | Fuel Pump Replacement

| for the 1.8L (L79) engine.

• | Fuel Pump Replacement for the 1.8L (LDA) engine.

• | Fuel Pump Replacement for the 2.0L engine.

Did you complete the repair?

--

Go to Step 7

--

6 | Replace the instrument cluster assembly. Refer to Instrument Cluster Replacement . Did you complete the repair? | -- | Go to Step 7 | --
7 | Operate the system in order to verify the repair. Did you find and complete the repair? | -- | System OK | Go to Step 2