For 1990-2009 cars

### Removal Procedure

Caution: Refer to Vehicle Lifting Caution in the Preface section.

1. Raise and suitably support the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Remove the front wheel. Refer to Tire and Wheel Removal and Installation .
3. Remove the front mud guard. Refer to Rear Mud Flap Guard Replacement .
4. Remove the screws and the front wheel well splash shield.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the screws and the front wheel well splash shield.

Tighten
Tighten the front wheel well splash shield screws to 2 N·m (18 lb in).

2. Install the front mud guard. Refer to Rear Mud Flap Guard Replacement .
3. Install the front wheel. Refer to Tire and Wheel Removal and Installation .
4. Lower the vehicle.