For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Disconnect the evaporative emission (EVAP) canister front hose from the EVAP emission purge solenoid valve.
3. Disconnect the EVAP emission canister front hose from the EVAP emission canister pipe.
4. Disconnect the EVAP emission canister pipe from the EVAP emission canister rear hose.
5. Remove the EVAP canister pipe retaining bolts.
6. Remove the EVAP canister pipe.

### Installation Procedure

1. Position the EVAP canister pipe to the vehicle.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the EVAP canister pipe retaining bolts.

Tighten
Tighten the EVAP canister pipe retaining bolts to 10 N·m (7 lb ft).

3. Connect the EVAP emission canister pipe to the EVAP emission canister rear hose.
4. Connect the EVAP emission canister front hose to the EVAP emission canister pipe.
5. Connect the EVAP canister front hose to the EVAP emission purge solenoid valve.
6. Connect the negative battery cable.