For 1990-2009 cars

### Circuit Description

When the ignition switch is turned to ON, the sensing and diagnostic module (SDM) will perform a turn-on test to diagnose critical malfunctions within the SDM itself.

These test ignition and deployment loop voltages are measured to ensure that they are within their normal voltage ranges. The SDM monitors the voltages at the driver low and the passenger low to detect shorts to ground or voltage in the deployment loops.

The SDM inspects the wiring connection to the driver belt pretensioner module by letting the perpetual current flow through the internal circuit and verify the resistance.

### DTC Descriptor

This diagnostic procedure supports the following DTC:

DTC B1361 Driver Pretensioner Deployment Resistance High

### Conditions for Running the DTC

Ignition voltage is within the normal operating voltage range.

### Conditions for Setting the DTC

The resistance of the driver belt pretensioner deploy loop is over 3 ohms.

### Action Taken When the DTC Sets

The SDM commands the AIR BAG indicator ON.

### Conditions for Clearing the DTC

The condition responsible for setting the DTC no longer exists and the scan tool Clear DTCs function is used.

Step | Action | Values | Yes | No
--- | --- | --- | --- | ---
Caution: Refer to Sensing and Diagnostic Module Handling Caution in the Preface section. Caution: Refer to Sensing and Diagnostic Module Voltage after Ignition is Turned Off Caution in the Preface section. Schematic Reference: SIR Schematics Connector End View Reference: Component Connector End Views
1 | Did you perform the Diagnostic System Check - Vehicle? | -- | Go to Step 2 | Go to Diagnostic System Check - Vehicle
2 | Visually inspect the wiring of the driver belt pretensioner. Is the wiring damaged? | -- | Go to Step 5 | Go to Step 3
3 |

1. Confirm the ignition switch is OFF.
2. Disconnect the connector of the drive belt pretensioner.
3. Disconnect the connector of the sensing and diagnostic module (SDM) wiring.
4. Measure the resistance between terminal 33, 34 of the SDM connector and terminal 2, 1 of the driver belt pretensioner connector respectively.

Is the resistance equal to the specified value?

0 ohms

Go to Step 4

Go to Step 5

4 |

1. Replace the SDM. Refer to Inflatable Restraint Sensing and Diagnostic Module Replacement .
2. Confirm the ignition switch is ON.
3. Erase the DTC using the scan tool.
4. Perform the Diagnostic System Check - Vehicle .

Is the DTC removed?

--

Go to Step 7

Go to Step 6

5 | Replace the air bag wiring. Is the replacement complete? | -- | Go to Step 7 | --
6 | Replace the driver belt pretensioner. Refer to Front Seat Belt Replacement . Is the replacement complete? | -- | Go to Step 7 | --
7 |

1. Reconnect all SIR components.
2. Verify that all components, connectors and connector position assurances (CPAs) are properly mounted.
3. Use the scan tool in order to clear the DTCs.
4. Operate the vehicle within the Conditions for Running the DTC, as specified in the supporting text.

Does the DTC reset?

--

Go to Step 2

System OK