For 1990-2009 cars

### Removal Procedure

1. Open the liftgate
2. Remove the rear compartment lower cover. Refer to Rear Compartment Trim Panel Replacement.
3. Remove the bolts securing the lock striker.
4. Pull the lock striker out.
5. Disconnect the lock release cable from the lock striker.

### Installation Procedure

1. Connect the lock release cable.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the lock striker with the bolts and tighten to 20 N·m (15 lb ft).
3. Install the rear compartment lower cover. Refer to Rear Compartment Trim Panel Replacement.