For 1990-2009 cars

## Fluid and Lubricant Recommendations Except Holden

Usage | Capacity | Fluid/Lubricant
--- | --- | ---
Automatic Transaxle

- 1.6L DOHC (Aisin 81-40LE)

5.77 ± 0.2L (6.1 ± 0.2 qt)

ESSO JWS 3309 or Total Fluid III G

- 1.8L/2.0L DOHC (ZF 4HP16)

6.9 ± 0.2L (7.3 ± 0.2 qt)

ESSO LT 71141 or Total ATF H50235

Automatic Transaxle Shift Linkage | As Required | Engine Oil
Brake Fluid and Clutch Fluid | 0.5L (0.5 qt) | DOT-3 or DOT-4
Clutch Linkage Pivot Points | As Required | Engine Oil
Engine Coolant

- 1.4L DOHC

7.2L (7.6 qt)

Mixture of water and good quality silicate base antifreeze (year-round coolant)

- 1.6L DOHC

7.2L (7.6 qt)

Mixture of water and good quality silicate base antifreeze (year-round coolant)

- 1.8L/2.0L DOHC

7.5L (7.9 qt)

Mixture of water and good quality silicate base antifreeze (year-round coolant)

Engine Oil

- 1.4L DOHC

3.75L (3.96 qt)

API SL (ILSAC GF-III) Grade SAE5W-30 (Hot Area--SAE10W-30)

- 1.6L DOHC

3.75L (3.96 qt)

API SL (ILSAC GF-III) Grade SAE5W-30 (Hot Area--SAE10W-30)

- 1.8L/2.0L DOHC

4.0L (4.2 qt)

API SL (ILSAC GF-III) Grade SAE5W-30 (Hot Area--SAE10W-30)

Floor Shift Linkage Points | As Required | Engine Oil
Hood and Door Hinges Fuel Door Hinge Rear Compartment Lid Hinges | As Required | Engine Oil
Hood Latch Assembly

- Pivots and Spring Anchor

As Required

Engine Oil

- Release Pawl

As Required

Multipurpose type grease meeting requirements NLGI No. 1 or 2

Key Lock Cylinders | As Required | Silicone Lubricant
Manual Transaxle | 1.8L (2.0 qt) | SAE80W (Extremely Cold Area--SAE 75W)
Manual Transaxle Shift Linkage | As Required | Multipurpose type grease meeting requirements NLGI No. 1 or 2
Power Steering System | 1.1L (1.2 qt) | DEXRON® III or DEXRON® IID
Weatherstrips | As Required | Silicone Grease

## Fluid and Lubricant Recommendations Holden

Application | Fluid/Lubricant
--- | ---
Automatic Transaxle | ESSO LT 71141
Automatic Transaxle Shift Linkage | Engine Oil
Brake Fluid and Clutch Fluid | DOT-4
Clutch Linkage Pivot Points | Engine Oil
Engine Coolant | Silicate based coolant (blue)
Engine Oil |

• | SAE 5W-30 or 10W-30

• | API SL or SM

• | ILSAC GF-3 or GF-4

Floor Shift Linkage Points | Engine Oil
Hood and Door Hinges Fuel Door Hinge Rear Compartment Lid Hinges | Engine Oil
Hood Latch Assembly

- Pivots and Spring Anchor

Engine Oil

- Release Pawl

Multipurpose type grease meeting requirements NLGI No. 1 or 2

Key Lock Cylinders | Silicone Lubricant
Manual Transaxle | SAE 75W-90
Manual Transaxle Shift Linkage | Multipurpose type grease meeting requirements NLGI No. 1 or 2
Power Steering System | DEXRON® III
Weatherstrips | Silicone Grease