For 1990-2009 cars

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the front wheel well splash shields. Refer to Wheelhouse Splash Shield Replacement.
3. Remove the fog lamps and the headlamps. Refer to Front Fog Lamp Replacement and Headlamp Replacement.
4. Remove the fender-to-fascia bolts and the screws.
5. Remove the lower fascia screws and the bolts.
6. Remove the upper fascia screws.
7. Remove the front bumper fascia.

### Installation Procedure

1. Install the front bumper fascia.
2. Install the upper fascia screws.

Caution: Refer to Fastener Caution in the Preface section.

3. Install the bolts and the lower fascia screws and tighten to 2 N·m (18 lb in).
4. Install the fender-to-fascia bolts and the screws and tighten.

• | fender-to-fascia bolts to 10 N·m (89 lb in).

• | fender-to-fascia screws to 2 N·m (18 lb in).

5. Install the headlamps and the fog lamps. Refer to Headlamp Replacement and Front Fog Lamp Replacement.
6. Install the front wheel well splash shields. Refer to Wheelhouse Splash Shield Replacement.
7. Connect the negative battery cable.