For 1990-2009 cars

#### Tools Required

J 22610 Keystone Clamp Pliers

### Removal Procedure

Caution: Refer to Vehicle Lifting Caution in the Preface section.

1. Raise and suitably support the vehicle.
2. Remove the wheels. Refer to Tire and Wheel Removal and Installation .
3. Remove the outer tie rod. Refer to Rack and Pinion Outer Tie Rod End Replacement .
4. Remove the dust boot retaining clamps.
5. Remove the dust boot.

### Installation Procedure

1. Install the dust boot.
2. Install the tie rod end dust boot retaining clamp.

Install the cylinder end dust boot retaining clamp with J 22610 .

3. Install the outer tie rod. Refer to Rack and Pinion Outer Tie Rod End Replacement .
4. Install the wheel. Refer to Tire and Wheel Removal and Installation .
5. Lower the vehicle.