For 1990-2009 cars

### Removal Procedure

Warning: Refer to Sensing and Diagnostic Module Voltage after Ignition is Turned Off Warning in the Preface section.

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the glove box. Refer to Instrument Panel Storage Compartment Replacement.
3. Disconnect the passenger air bag yellow electrical connector.
4. Remove the instrument panel (I/P) module by removing the mounting bolts from the air bag bracket.

### Installation Procedure

1. Install the I/P module to the I/P.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the I/P module mounting bolts and tighten to 11 N·m (97 lb in.
3. Connect the passenger air bag yellow electrical connector.
4. Install the glove box. Refer to Instrument Panel Storage Compartment Replacement.
5. Connect the negative battery cable.