For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

Caution: Fuel Vapors can collect while servicing fuel system parts in enclosed areas such as a trunk. To reduce the risk of fire and increased exposure to vapors:

• | Use forced air ventilation such as a fan set outside of the trunk.

• | Plug or cap any fuel system openings in order to reduce fuel vapor formation.

• | Clean up any spilled fuel immediately.

• | Avoid sparks and any source of ignition.

• | Use signs to alert others in the work area that fuel system work is in process.

1. Disconnect the negative battery cable.
2. Remove the fuel tank. Refer to Fuel Tank Replacement .
3. Disconnect the canister fuel vapor hoses.
4. Remove the tie from the canister.
5. Remove the canister.

### Installation Procedure

1. Install the new tie from the canister.
2. Connect the canister fuel vapor hoses.
3. Install the fuel tank. Refer to Fuel Tank Replacement .
4. Connect the negative battery cable.