For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the instrument cluster trim panel.
3. Remove the screws and the instrument cluster.
4. Disconnect the electrical connectors.

### Installation Procedure

1. Connect the electrical connectors.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the instrument cluster with the screws.

Tighten
Tighten the instrument cluster screw to 4 N·m (35 lb in).

3. Install the instrument cluster trim panel.
4. Connect the negative battery cable.