For 1990-2009 cars

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the negative battery cable.
2. Pry off the interior courtesy lamp lens.
3. Remove the screws and the switch.
4. Disconnect the electrical connector.

### Installation Procedure

1. Connect the electrical connector.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the sunroof control switch with the screws and tighten to 2 N·m (18 lb in).
3. Install the interior courtesy lamp lens.
4. Connect the negative battery cable.