For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Disconnect the intake air temperature (IAT) sensor connector.
3. Disconnect the air cleaner outlet hose from the throttle body.
4. Disconnect the breather tube from the camshaft cover.
5. Remove the air cleaner housing bolts.
6. Remove the air cleaner housing.
7. Remove the right front wheel. Refer to Tire and Wheel Removal and Installation.
8. Remove the right front wheel well splash shield. Refer to Wheelhouse Splash Shield Replacement .
9. Remove the serpentine accessory drive belt. Refer to Power Steering Pump Belt Replacement.
10. Remove the crankshaft pulley bolts.
11. Remove the crankshaft pulley.
12. Remove the right engine mount bracket. Refer to Engine Mount Replacement .
13. Remove the front timing belt cover bolts.
14. Remove the front timing belt cover.
15. Using the crankshaft gear bolt, rotate the crankshaft clockwise until the timing mark on the crankshaft gear is aligned with the notch at the bottom of the rear timing belt cover.

Important: The camshaft gears must align with the notch on the camshaft cover or damage to the engine could result.

Important: Use the intake gear mark for the intake camshaft gear and the exhaust gear mark for the exhaust camshaft gear since both gears are interchangeable.

16. Align the camshaft gear notch (1, 2) with the notch on the camshaft cover.
17. Loosen the automatic tensioner bolt. Turn the hex-key tab to relieve belt tension.
18. Remove the timing belt.

### Installation Procedure

1. Align the timing mark on the crankshaft gear with the notch on the bottom of the rear timing belt cover.
2. Align the timing marks on the camshaft gears, using the intake gear mark (1) for the intake gear and the exhaust gear mark (2) for the exhaust gear.
3. Install the timing belt.
4. Turn the hex-key tab in a clockwise direction to tension the belt. Turn until the pointer aligns with the notch.

Notice: Refer to Fastener Notice in the Preface section.

5. Install the automatic tensioner bolt.

Tighten
Tighten the automatic tensioner bolt to 25 N·m (18 lb ft).

6. Rotate the crankshaft 2 full turns clockwise using the crankshaft pulley bolt.
7. Recheck the automatic tensioner pointer.
8. Install the front timing belt cover.
9. Install the front timing belt cover bolts.

Tighten
Tighten the front timing belt cover bolts to 6 N·m (53 lb in).

10. Install the right engine mount bracket. Refer to Engine Mount Replacement .
11. Install the crankshaft pulley.
12. Install the crankshaft pulley bolts.

Tighten
Tighten the crankshaft pulley bolts to 20 N·m (15 lb ft).

13. Install the serpentine accessory drive belt. Refer to Power Steering Pump Belt Replacement.
14. Install the right front wheel well splash shield. Refer to Wheelhouse Splash Shield Replacement.
15. Install the right front wheel. Refer to Tire and Wheel Removal and Installation.
16. Install the air cleaner housing.
17. Install the air cleaner housing bolts.

Tighten
Tighten the air cleaner housing bolts to 10 N·m (89 lb in).

18. Connect the air cleaner outlet hose to the throttle body.
19. Connect the breather tube to the camshaft cover.
20. Connect the IAT sensor connector.
21. Connect the negative battery cable.