For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Rear Brake Drums

- Inside Diameter - New

200 mm

7.87 in

- Maximum Rebore Diameter

201 mm

7.91 in

- Radial Runout - Not Installed

0.04 mm

0.0016 in

Booster Size

- Single

241.3 mm

9.5 in

- Dual

177.8 and 203.2 mm

7 and 8 in

Booster Ratio | 5.5:1
Caliper

- Minimum Piston Diameter - Front

54 mm

2.126 in

- Minimum Piston Diameter - Rear

32 mm

1.260 in

Front Brake Rotors

- Disc Type

Ventilated

- Discard Thickness

22 mm

0.87 in

- Lateral Runout - Installed

0.06 mm

0.002 in

- Lateral Runout - Not Installed

0.03 mm

0.001 in

- Rotor Diameter

256 mm

10.07 in

- Rotor Thickness - New

24 mm

0.95 in

- Thickness Variation

0.01 mm

0.0004 in

Master Cylinder

- Bore Diameter - Nominal

22.22 mm

0.875 in

- Bore Diameter - Maximum

22.29 mm

0.878 in

Rear Brake Rotors

- Disc Type

Solid

- Discard Thickness

8 mm

0.31 in

- Lateral Runout - Installed

0.08 mm

0.003 in

- Lateral Runout - Not Installed

0.05 mm

0.002 in

- Rotor Diameter

258 mm

10.15 in

- Rotor Thickness - New

10.4 mm

0.40 in

- Thickness Variation

0.01 mm

0.0004 in

Wheel Cylinder Diameter

- Maximum

20.7 mm

0.815 in

- Nominal

20.64 mm

0.812 in