For 1990-2009 cars

#### Special Tools

J 21104-B (KM-475-B) Weatherstrip Remover Universal

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the sunroof molding, if equipped.
3. Remove the passenger assist handles. Refer to Assist Handle Replacement.
4. Remove the plastic retaining clips in the headliner on the driver side.
5. Remove the sun visors. Refer to Sunshade Replacement.
6. Remove the power sunroof control switch, if equipped. Refer to Sunroof Switch Replacement.
7. Remove the windshield pillar. Refer to Windshield Pillar Garnish Molding Replacement.
8. Remove the upper center pillar. Refer to Center Pillar Upper Trim Panel Replacement.
9. Remove the plastic retainers in the headliner using the J 21104-B .
10. Recline both front seats.
11. Remove the headliner.
12. Remove the rear quarter upper trim panel. Refer to Quarter Upper Trim Panel Replacement.

### Installation Procedure

1. Recline both front seats.
2. Install the headliner behind the seats around the doors.
3. Install the plastic retainers.
4. Install the windshield pillar. Refer to Windshield Pillar Garnish Molding Replacement.
5. Install the upper center pillar. Refer to Center Pillar Upper Trim Panel Replacement.
6. Install the rear quarter upper trim panel. Refer to Quarter Upper Trim Panel Replacement.
7. Install the power sunroof control switch, if equipped. Refer to Sunroof Switch Replacement.
8. Install the sun visors. Refer to Sunshade Replacement.
9. Install the plastic retainers in the headliner on the driver side.
10. Install the passenger assist handles. Refer to Assist Handle Replacement.
11. Install the sunroof molding, if equipped.
12. Connect the negative battery cable.