For 1990-2009 cars

#### Tools Required

DT 46475 (DW260-070) Auto Transaxle Oil Plug Remover/Installer

Notice: Refer to Fastener Notice in the Preface section.

1. Install the oil pan and the oil pan gasket and the bolts.

Tighten
Tighten the bolts to 6 N·m (53 lb in).

2. Install the oil cooler inlet and outlet pipes. Refer to Transmission Fluid Cooler Hose/Pipe Replacement .
3. Use DT 46475 (1) to install the transaxle fluid drain plug.
4. Install the engine cover. Refer to Engine Cover Replacement.
5. Refill the transaxle fluid. Refer to Transmission Fluid Level Inspection .
6. Connect the negative battery cable.