For 1990-2009 cars

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.
2. Remove the left knee bolster. Refer to Knee Bolster Replacement.
3. Disconnect the connector (2) of the object alarm control module (3).
4. Remove the screws (1) and the rear object alarm control module (3).

### Installation Procedure

1. Install the rear object alarm control module (3) with the screws (1).
2. Connect the electrical connectors (2).
3. Install the knee bolster. Refer to Knee Bolster Replacement.
4. Connect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.