For 1990-2009 cars

### Removal Procedure

1. Remove the timing belt and the timing belt cover. Refer to Timing Belt Replacement .
2. Remove the camshaft gears. Refer to Camshaft Gear Replacement .
3. Remove the crankshaft gear.
4. Remove the timing belt automatic tensioner bolts.
5. Remove the timing belt automatic tensioner.
6. Remove the timing belt idler pulley bolt.
7. Remove the timing belt idler pulley.
8. Remove the rear timing belt cover bolts.
9. Remove the rear timing belt cover.

### Installation Procedure

1. Install the rear timing belt cover.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the rear timing belt cover bolts.

Tighten
Tighten the rear timing belt cover bolts to 10 N·m (89 lb in).

3. Install the timing belt idler pulley.
4. Install the timing belt idler pulley bolt.

Tighten
Tighten the timing belt idler pulley bolt to 40 N·m (30 lb ft).

5. Install the timing belt automatic tensioner.
6. Install the timing belt automatic tensioner bolts.

Tighten
Tighten the timing belt automatic tensioner bolts to 25 N·m (18 lb ft).

7. Install the crankshaft gear.
8. Install the camshaft gears. Refer to Camshaft Gear Replacement .
9. Install the timing belt and timing belt cover. Refer to Timing Belt Replacement .