For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the instrument cluster. Refer to Instrument Cluster Replacement .
3. Remove the defective bulb from the rear of the cluster.

### Installation Procedure

1. Install the new bulb.
2. Install the instrument cluster. Refer to Instrument Cluster Replacement .
3. Connect the negative battery cable.