For 1990-2009 cars

### Circuit Description

When the ignition switch is turned to ON, the sensing and diagnostic module (SDM) will perform a turn-on test to diagnose critical malfunctions within the SDM itself.

If driver side impact module inflation was caused by side impact, the SDM maintains warning lamp ON and the entire air bag system should be inspected, including pretensioners. The side air bag sensor and wiring should be replaced. If the driver side impact module inflation by side impact counts over 5, the SDM should also be replaced.

### DTC Descriptor

This diagnostic procedure supports the following DTC:

DTC 033 Driver Side Airbag Inflation Record By Side Impact

### Conditions for Running the DTC

Ignition voltage is within the normal operating voltage range.

### Conditions for Setting the DTC

The history of the air bag inflation or belt pretensioner deploment is in the SDM.

### Action Taken When the DTC Sets

The SDM commands the AIR BAG indicator ON.

### Conditions for Clearing the DTC

The condition responsible for setting the DTC no longer exists and the scan tool Clear DTCs function is used.

Step | Action | Yes | No
--- | --- | --- | ---
Caution: Refer to Sensing and Diagnostic Module Voltage after Ignition is Turned Off Caution in the Preface section. Caution: Refer to Sensing and Diagnostic Module Handling Caution in the Preface section. Schematic Reference: SIR Schematics Connector End View Reference: SIR Connector End Views
1 | Did you perform the Diagnostic System Check - Vehicle? | Go to Step 2 | Go to Diagnostic System Check - Vehicle
2 |

1. Disconnect the negative battery cable.
2. Wait 1 minute for the sensing and diagnostic module (SDM) capacitor to discharge.
3. Visually inspect the supplemental inflatable restraints (SIR) wiring harness.

Is there any visible damage to the SIR harness?

Go to Step 4

Go to Step 3

3 | Replace the SDM. Refer to Inflatable Restraint Sensing and Diagnostic Module Replacement. Did you complete the repair? | Go to Step 5 | --
4 | Replace the SIR wiring harness. Did you complete the repair? | Go to Step 5 | --
5 |

1. Reconnect all SIR components.
2. Verify that all components, connectors and connector position assurances (CPAs) are properly mounted.
3. Use the scan tool in order to clear the DTCs.
4. Operate the vehicle within the Conditions for Running the DTC, as specified in the supporting text.

Does the DTC reset?

Go to Step 2

System OK