For 1990-2009 cars

### Removal Procedure

Caution: Refer to Sensing and Diagnostic Module Voltage after Ignition is Turned Off Caution in the Preface section.

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the trim from the center pillar.
3. Disconnect the side impact sensor connector (2).
4. Remove the side impact sensor mounting bolts.
5. Remove the side impact sensor (1).

### Installation Procedure

1. Install the side impact sensor (1).

Notice: Refer to Fastener Notice in the Preface section.

2. Install the side impact sensor mounting bolts.

Tighten
Tighten the side impact sensor mounting bolts to 8 N·m (71 lb in).

3. Connect the side impact sensor connector (2).
4. Install the trim to the center pillar.
5. Connect the negative battery cable.