For 1990-2009 cars

### Removal Procedure

1. Disconnect the speedometer speed sensor electrical connector.
2. Remove the speedometer housing retaining bolt.
3. Remove the speedometer-driven gear and the speedometer housing.

### Installation Procedure

1. Coat the O-ring with petroleum jelly.
2. Install the speedometer-driven gear and the speedometer housing.

Caution: Refer to Fastener Caution in the Preface section.

3. Install the speedometer housing retaining bolt and tighten to 5 N·m (44 lb in).
4. Connect the speedometer speed sensor electrical connector.