For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the deposit box. Refer to Deposit Box Replacement in Instrument Panel, Gages, and Console.
3. Remove the bolt.
4. Disconnect the electrical connector.
5. Remove the folding mirror switch.

### Installation Procedure

1. Connect the electrical connector.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the folding mirror switch with the bolt.

Tighten
Tighten the daytime running lamp module bolts to 10 N·m (89 lb in).

3. Install the deposit box. Refer to Deposit Box Replacement in Instrument Panel, Gages, and Console.
4. Connect the negative battery cable.