For 1990-2009 cars

1. The power steering fluid level is indicated either by marks on a see-through fluid reservoir or by marks on a fluid level indicator on the fluid reservoir cap.

Notice: Refer to Using Proper Power Steering Fluid Notice in the Preface section.

2. If the fluid is warmed up to 66°C (150°F), the fluid level should be between the MAX and MIN marks. Add fluid if necessary.
3. If the fluid is cool, 21°C (70°F), the fluid level should be at the MIN mark. Add fluid if necessary.