For 1990-2009 cars

### Removal Procedure

1. Raise the hood and support it with the hood prop.
2. Remove the weatherstrip.
3. Remove the wiper arms. Refer to Windshield Wiper Arm Replacement .
4. Remove the air inlet grille panel screws and the 2-piece grille.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the 2-piece grille and the air inlet grille screws.

Tighten
Tighten the air inlet grille screws to 4 N·m (35 lb in).

2. Remove the wiper arms. Refer to Windshield Wiper Arm Replacement .
3. Install the weatherstrip.