For 1990-2009 cars

Table 1: | Camshaft Position (CMP) Sensor
Table 2: | Crankshaft Position Sensor (CKP) Sensor
Table 3: | Engine Coolant Temperature (ECT) Sensor
Table 4: | Evaporative Emissions (EVAP) Canister Purge Solenoid Valve
Table 5: | Exhaust Gas Recirculation (EGR) Valve (ECE 83 Emissions)
Table 6: | Exhaust Gas Recirculation (EGR) Valve (Euro III Emissions)
Table 7: | Exhaust Gas Recirculation (EGR) Valve (Euro IV Emissions)
Table 8: | Fuel Injector 1
Table 9: | Fuel Injector 2
Table 10: | Fuel Injector 3
Table 11: | Fuel Injector 4
Table 12: | Fuel Pump/Sender
Table 13: | Heated Oxygen Sensor (HO2S) 1
Table 14: | Heated Oxygen Sensor (HO2S) 2
Table 15: | Ignition Coil Module (1 and 4)
Table 16: | Ignition Coil Module (2 and 3)
Table 17: | Intake Air Temperature (IAT) Sensor
Table 18: | Intake Manifold Tuning Valve
Table 19: | Knock Sensor (KS)
Table 20: | Manifold Absolute Pressure (MAP) Sensor
Table 21: | Octane Selection Switch
Table 22: | Oxygen (O2) Sensor
Table 23: | Rough Road Sensor
Table 24: | Throttle Body

#### Camshaft Position (CMP) Sensor

Connector Part Information |

• | AMP 85205-1

• | 3-Way F JR Power Timer 3P Hsg Ass'y (BK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | PK/BK | 1846 | Ignition 1 Voltage
2 | GY | 632 | Low Reference
3 | BN/WH | 633 | Camshaft Position (CMP) Sensor Signal

#### Crankshaft Position Sensor (CKP) Sensor

Connector Part Information |

• | AMP 85205-1

• | 3-Way F JR Power Timer 3P Hsg Ass'y (BK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | YE/BK | 1868 | Low Reference
2 | D-BU/WH | 1869 | Crankshaft Position (CKP) Sensor Signal
3 | BK/WH | 51 | Ground

#### Engine Coolant Temperature (ECT) Sensor

Connector Part Information |

• | PED 12040753

• | 2-Way F Metri-Pack 150 Series, Sealed, Pull To Seat (BK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | YE | 410 | Engine Coolant Temperature (ECT) Sensor Signal
2 | BK/YE | 808 | Low Reference

#### Evaporative Emissions (EVAP) Canister Purge Solenoid Valve

Connector Part Information |

• | AMP 85202-1

• | 2-Way F JR Power Timer 2P Hsg Ass'y (BK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | PK/BK | 1846 | Ignition 1 Voltage
2 | D-GN/WH | 428 | EVAP Canister Purge Solenoid Control

#### Exhaust Gas Recirculation (EGR) Valve (ECE 83 Emissions)

Connector Part Information |

• | AMP 368530

• | 2-Way M Econoseal J Mark II + Connector Plug Housing (BK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | GY | 435 | Exhaust Gas Recirculation (EGR) Solenoid Control
2 | PK | 139 | Ignition 1 Voltage

#### Exhaust Gas Recirculation (EGR) Valve (Euro III Emissions)

Connector Part Information |

• | AMP 368530-1

• | 6-Way F Econoseal J-Mark II + 6P (BK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | GY | 416 | 5-Volt Reference Voltage
2 | BK/YE | 808 | Sensor Ground
3 | BN | 1456 | Exhaust Gas Recirculation (EGR) Signal
4 | PK | 139 | Ignition 1 Voltage
5 | -- | -- | Not Used
6 | GY | 435 | Exhaust Gas Recirculation (EGR) Solenoid Low Control

#### Exhaust Gas Recirculation (EGR) Valve (Euro IV Emissions)

Connector Part Information |

• | AMP 368530-1

• | 6-Way F Econoseal J-Mark II + 6P (BK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | GY | 435 | Exhaust Gas Recirculation (EGR) Solenoid Low Control
2 | BK/YE | 808 | Sensor Ground
3 | BN | 1456 | Exhaust Gas Recirculation (EGR) Signal
4 | GY | 416 | 5-Volt Reference Voltage
5 | PK | 139 | Ignition 1 Voltage
6 | -- | -- | Not Used

#### Fuel Injector 1

Connector Part Information |

• | AMP 85202-1

• | 2-Way F JR Power Timer 2P Hsg Ass'y (BK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | PK | 139 | Ignition 1 Voltage
2 | BK | 1744 | Fuel Injector 1 Control

#### Fuel Injector 2

Connector Part Information |

• | AMP 85202-1

• | 2-Way F JR Power Timer 2P Hsg Ass'y (BK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | PK | 139 | Ignition 1 Voltage
2 | L-GN/BK | 1745 | Fuel Injector 2 Control

#### Fuel Injector 3

Connector Part Information |

• | AMP 85202-1

• | 2-Way F JR Power Timer 2P Hsg Ass'y (BK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | PK | 139 | Ignition 1 Voltage
2 | PK/BK | 1746 | Fuel Injector 3 Control

#### Fuel Injector 4

Connector Part Information |

• | AMP 85202-1

• | 2-Way F JR Power Timer 2P Hsg Ass'y (BK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | PK | 139 | Ignition 1 Voltage
2 | L-BU/BK | 844 | Fuel Injector 4 Control

#### Fuel Pump/Sender

Connector Part Information |

• | AMP 936039

• | 6-Way F Fuel Pump 6POS Conn'r Ass'y (BN)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | D-BU | 1936 | Fuel Level Sensor Signal
2 | BK | 1250 | Ground
3 | GY | 120 | Fuel Pump Supply Voltage
4 | BK | 1250 | Ground
5 | PU | 172 | Low Fuel Indicator Control
6 | PU/BK | 632 | Low Reference

#### Heated Oxygen Sensor (HO2S) 1

Connector Part Information |

• | AMP 174257-2

• | 4-Way M 070 Series Econoseal J MK-2 Plug Ass'y 4P (BK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | PU/WH | 1665 | Heated Oxygen Sensor (HO2S) 1 Low Reference
2 | PK/BK | 1846 | Ignition 1 Voltage
3 | OG/BK | 469 | Heated Oxygen Sensor (HO2S) 1 Heater Control
4 | BN/WH | 1666 | Heated Oxygen Sensor (HO2S) 1 Signal

#### Heated Oxygen Sensor (HO2S) 2

Connector Part Information |

• | AMP 174257-2

• | 4-Way M 070 Series Econoseal J MK-2 Plug Ass'y 4P (BK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | PU | 1670 | Heated Oxygen Sensor (HO2S) 2 Low Reference
2 | PK/BK | 1846 | Ignition 1 Voltage
3 | L-GN | 413 | Heated Oxygen Sensor (HO2S) 2 Heater Control
4 | BN/BK | 1671 | Heated Oxygen Sensor (HO2S) 2 Signal

#### Ignition Coil Module (1 and 4)

Connector Part Information |

• | KET MG 641789-4

• | 2-Way F 090-II WP Series

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | OG | 406 | Ignition Coil Control (1 and 4)
2 | PK | 739 | Ignition 1 Voltage

#### Ignition Coil Module (2 and 3)

Connector Part Information |

• | KET MG 641637-5

• | 2-Way F 090-II WP Series (BK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | WH | 423 | Ignition Coil Control (2 and 3)
2 | PK | 739 | Ignition 1 Voltage

#### Intake Air Temperature (IAT) Sensor

Connector Part Information |

• | AMP 85202-1

• | 2-Way F JR Power Timer 2P Hsg Ass'y (BK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BN | 472 | Intake Air Temperature (IAT) Sensor Signal
2 | OG/BK | 469 | Low Reference

#### Intake Manifold Tuning Valve

Connector Part Information |

• | AMP 174352-2

• | 2-Way M Econoseal J Mark II + Connector Plug Housing (BK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | WH/BK | 962 | Intake Manifold Tuning Valve Solenoid Control
2 | PK/BU | 539 | Ignition 1 Voltage

#### Knock Sensor (KS)

Connector Part Information |

• | AMP 368215-1

• | 3-Way F JPT 3P Ass'y for Knock Sensor (GY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | YE/BK | 496 | Knock Sensor (KS) Signal
2 | D-BU/WH | 1876 | Low Reference
3 | BK/WH | 51 | Ground

#### Manifold Absolute Pressure (MAP) Sensor

Connector Part Information |

• | PED 12129946

• | 3-Way F Metri-Pack 150 Series Sealed (GY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | OG/BK | 469 | Low Reference
B | L-GN | 432 | Manifold Absolute Pressure (MAP) Sensor Signal
C | L-BU/BK | 1688 | 5-Volt Reference

#### Octane Selection Switch

Connector Part Information |

• | KET MG 640329

• | 3-Way M SWP Series (BK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | PU | 773 | Octane Switch Signal
2 | BK/WH | 251 | Ground
3 | L-BU | 772 | Octane Switch Signal

#### Oxygen (O2) Sensor

Connector Part Information |

• | AMP 174352-2

• | 2-Way M Econoseal J Mark II + Connector Plug Housing (BK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | PU/WH | 1665 | Oxygen (O2) Sensor Signal
2 | OG/BK | 469 | Low Reference

#### Rough Road Sensor

Connector Part Information |

• | Bosch 2264-420424

• | 2-Way F Metri-Pack 150 Series, Sealed (GY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | WH | 873 | Rough Road Sensor Signal
B | OG | 830 | 5-Volt Reference

#### Throttle Body

Connector Part Information |

• | AMP 174982-2

• | 8-Way F 070 Series Econoseal J-Mark II + 8P (BK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | D-BU | 426 | Idle Motor Return
2 | GY | 416 | 5-Volt Reference
3 | -- | -- | Not Used
4 | D-GN | 534 | High Idle Switch Signal
5 | L-BU | 425 | Idle Motor Feed
6 | PK | 427 | Idle Speed Motor Switch Signal
7 | D-BU | 417 | Throttle Position (TP) Sensor Signal
8 | BK/YE | 808 | Low Reference