For 1990-2009 cars

## Headlamp Replacement Four Door/Wagon

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the headlamp mounting bolts.
3. Remove the headlamp mounting nut.
4. Disconnect the turn signal electrical connector.
5. Disconnect the headlamp electrical connector.
6. Remove the headlamp assembly.
7. Turn left and remove the headlamp bulb cap, if necessary.
8. Dry off the headlamp bulb clip.
9. Disconnect the headlamp bulb connector.
10. Remove the headlamp bulb, if necessary.
11. Remove the park lamp.
12. Remove the headlamp high beam cap.
13. Remove the headlamp high beam bulb clip.
14. Disconnect the headlamp high beam bulb connector.
15. Remove the headlamp high beam bulb, if necessary.
16. Remove the turn signal lamp, if necessary.

### Installation Procedure

1. Install the turn signal lamp, if removed.
2. Install the headlamp high beam bulb, if removed.
3. Connect the headlamp high beam bulb connector.
4. Install the headlamp high beam bulb clip.
5. Install the cap concealing the headlamp high beam bulb.
6. Install the park lamp.
7. Install the headlamp bulb, if removed.
8. Connect the headlamp bulb connector.
9. Install the headlamp bulb clip.
10. Turn to the right and install the headlamp bulb cap.
11. Install the headlamp assembly.
12. Connect the headlamp electrical connector.
13. Install the turn signal bulb, if removed.
14. Connect the turn signal connector.

Caution: Refer to Fastener Caution in the Preface section.

15. Install the headlamp mounting nut and tighten to 4 N·m (35 lb in).
16. Install the headlamp mounting bolts and tighten to 4 N·m (35 lb in).
17. Connect the negative battery cable.

## Headlamp Replacement Hatchback

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the radiator grille screws.
3. Insert a flat-bladed tool, into the radiator service hole and then push the radiator grille clips.
4. Remove the radiator grille.
5. Remove the headlamp mounting bolts.
6. Disconnect the parklamp electrical connector.
7. Disconnect the headlamp electrical connector.
8. Remove the headlamp assembly.
9. Turn left and remove the headlamp bulb cap, if necessary.
10. Pry off the headlamp bulb clip, if necessary.
11. Disconnect the headlamp bulb connector, if necessary.
12. Remove the headlamp bulb, if necessary.
13. Remove the park lamp, if necessary.
14. Remove the turn signal lamp, if necessary.

### Installation Procedure

1. Install the turn signal lamp, if removed.
2. Install the park lamp, if removed.
3. Install the headlamp bulb, if removed.
4. Install the headlamp bulb clip, if removed.
5. Connect the headlamp bulb electrical connector, if removed.
6. Install the cap concealing the headlamp bulb, if removed.
7. Install the headlamp assembly.
8. Connect the headlamp electrical connector.
9. Connect the park lamp electrical connector.

Caution: Refer to Fastener Caution in the Preface section.

10. Install the headlamp mounting bolts and tighten to 4 N·m (35 lb in).
11. Install the radiator grille.
12. Install the radiator grille screws.
13. Connect the negative battery cable.