For 1990-2009 cars

### Removal Procedure

1. Remove the cowl vent grille. Refer to Air Inlet Grille Panel Replacement.
2. Disconnect the windshield washer hose from the washer nozzles.
3. Remove the front left wheel. Refer to Tire and Wheel Removal and Installation.
4. Remove the bolts and the screws and the front wheel well splash shield.
5. Disconnect the washer hose from the washer reservoir.
6. Remove the washer hose.

### Installation Procedure

1. Install the washer hose.
2. Connect the washer hose to the washer pump.

Caution: Refer to Fastener Caution in the Preface section.

3. Install the front wheel well splash shield with the bolts and the screws and tighten to 1.5 N·m (13 lb in).
4. Install the front left wheel. Refer to Tire and Wheel Removal and Installation.
5. Connect the windshield washer hose to the washer nozzles.
6. Install the cowl vent grille. Refer to Air Inlet Grille Panel Replacement.