For 1990-2009 cars

### Removal Procedure

1. Disconnect the vacuum hose from the intake manifold tuning (IMT) valve actuator valve.

Note: Ensure the IMT valve is closed before removing the IMT valve actuator retaining bolts and valve.

2. Remove the IMT valve actuator valve bolts.
3. Remove the IMT valve actuator valve from the IMT valve.

### Installation Procedure

1. Install the IMT valve actuator valve to the IMT valve.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the IMT valve actuator valve bolts and tighten to 12 N·m (106 lb ft).
3. Connect the vacuum hose to the IMT valve actuator valve.