For 1990-2009 cars

## Relay Replacement Within an Electrical Center

#### Special Tools

J 43244 Relay Puller Pliers

### Removal Procedure

1. Remove the electrical center cover.
2. Locate the relay. Refer to Electrical Center Identification Views to locate the electrical center where the relay exists.

Important:

• | Always note the orientation of the relay.

• | If equipped with a notch style relay; observe the location of the notch on the old relay to verify the new relay is installed with the notch in the same location.

• | Ensure that the electrical center is secure, as not to put added stress on the wires or terminals.

3. Using the J 43244 (1) position the tool on opposing corners of the relay (2).

Notice: Use J43244 to pull the relay straight out from the electrical center terminals. The use of pliers or a flat bladed tool could damage the electrical center.

4. Remove the relay (2) from the electrical center.

### Installation Procedure

1. Install the relay (2) in the same position as removed.
2. Install the electrical center cover.