For 1990-2009 cars

Checks | Action
--- | ---
Inspect for a lack of lubrication of the ball joints and the tie rod ends. | Replace the ball joints and the outer tie rods.
Inspect for damaged suspension components. | Replace the damaged suspension components.
Inspect for worn control arm bushings or tie rod ends. | Replace the control arm bushings or the tie rods.
Inspect for a loose stabilizer shaft link. | Replace the stabilizer shaft link.
Inspect for loose wheel nuts | Tighten the wheel nuts.
Inspect for loose suspension bolts or nuts. | Replace worn front suspension components as needed.
Inspect for worn strut dampeners or strut mountings. | Replace the strut dampeners. Tighten the strut mounting bolts.
Inspect for an improperly positioned strut spring. | Adjust the strut spring to the proper position.