For 1990-2009 cars

1. Remove the rear quarter upper trim panel. Refer to Quarter Upper Trim Panel Replacement .
2. Remove the nuts and the rear door quarter glass.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the rear door quarter glass with the nuts.

Tighten
Tighten the rear door quarter glass nuts to 2.5 N·m (22 lb in).

2. Install the rear quarter upper trim panel. Refer to Quarter Upper Trim Panel Replacement .