For 1990-2009 cars

### Removal Procedure

Warning: Refer to Relieving Fuel Pressure Warning in the Preface section.

1. Relieve the fuel system pressure. Refer to Fuel Pump Replacement.

Warning: Refer to Battery Disconnect Warning in the Preface section.

2. Disconnect the negative battery cable.
3. Remove the rear seat. Refer to Rear Seat Cushion Replacement.
4. Remove the fuel pump access cover.
5. Disconnect the electrical connector at the fuel pump assembly.
6. Disconnect the fuel outlet line.
7. Disconnect the fuel tank return line.
8. Turn the lock ring counterclockwise to clear the tank tabs.
9. Remove the fuel pump assembly from the tank.

### Installation Procedure

Warning: Refer to Safety Glasses Warning in the Preface section.

1. Clean the gasket mating surface on the fuel tank.
2. Position the new gasket in place.
3. Install the fuel pump into the fuel tank in the same location as removed for ease of line and connector installation.
4. Position the lock ring in place and turn it clockwise until it contacts the tank stop.
5. Connect the fuel pump assembly connector.
6. Install the fuel pump outlet line.
7. Install the fuel tank return line.
8. Install the fuel pump access cover.
9. Connect the negative battery cable.
10. Perform an operational check of the fuel pump.
11. Install the rear seat. Refer to Rear Seat Cushion Replacement.