For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the knee bolster trim panel beneath the steering column.
3. Disconnect the electrical connector.
4. Remove the screws and the chime module.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the chime module with the screws.
2. Connect the electrical connector.
3. Install the knee bolster trim panel beneath the steering column.
4. Connect the negative battery cable.