For 1990-2009 cars

### Removal Procedure

1. Remove the stabilizer shaft-to-stabilizer link nut.
2. Remove the stabilizer link-to-strut assembly nut.
3. Remove the stabilizer link.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the stabilizer link.
2. Install the stabilizer link-to-strut assembly nut.

Tighten
Tighten the stabilizer shaft-to-stabilizer link nut to 47 N·m (35 lb ft).

3. Install the stabilizer shaft-to-stabilizer link nut.

Tighten
Tighten the stabilizer shaft-to-stabilizer link nut to 47 N·m (35 lb ft).